|  |  |  |  |
| --- | --- | --- | --- |
| 1 | adapter | 5-Port USB 2.0 Hub with Micro Port, PS4 Keyboard/Mouse Adapter for Dell, Asus, HP, MacBook, Surface, Xbox, Flash Drive, Printer, Camera | Wide Compatibility: The Quality Valley 4-Port USB Hub works with various devices like laptops, PCs, XBOX, PS4, flash drives, keyboards, mice, card readers, HDDs, OTG adapters, printers, cameras, USB fans, and cables.  USB 2.0 Super Speed: Featuring USB 3.0, this 4-port splitter supports up to 5 Gbps data transfer, backward compatible with USB 2.0/1.0. Tested speeds reach 371.19MB/s read, 245.97MB/s write (USB 3.0), and 43.18MB/s read, 40.84MB/s write (USB 2.0).  4 Ports Simultaneously: Provides stable performance for all 4 ports at once, with moderate temperature control.  Slim Design: Compact and designed with enough space between ports to fit multiple flash drives at once without crowding.  Premium PCB Quality: Years of expertise ensure no signal interference, even with WiFi or 2.4G during data transfers. Comes with a 30-day guarantee.  Customer Satisfaction: Quality Valley offers a 100% refund within 30 days for worry-free purchases. |
| 1 | cooler | Cooler Master MasterLiquid ML120L V2 RGB CPU Liquid Cooler - Enhanced Lighting, 3rd Gen Pump, Upgraded Radiator, and 120mm SickleFlow Fan, Black | Dimensions: LxWxH23.9 x 20.7 x 13.7 centimeters  Brand Cooler Master  Voltage: 12 Volts  Wattage: 3.36 watts  Compatible devices: Desktop  Noise level: 15 dB  Material: Aluminum  **About this item**  QUIETLY IMPROVED V2 RGB - Featuring brighter RGB lighting, enhanced cooling, and much quieter operation, the ML120L V2 RGB raises the standard for mainstream liquid coolers.  3RD GEN DUAL-CHAMBER PUMP - Equipped with a copper plate heat exchanger, the 3rd Gen dual-chamber pump offers increased water capacity, improved flow between chambers, and triple industrial-grade EPDM rubber gaskets for better performance.  25% LARGER RADIATOR SURFACE AREA - The 157 x 119.6 x 27 mm radiator features deeper fins than its predecessor, ensuring efficient heat dissipation through wider water channels.  ADVANCED SICKLEFLOW 120 RGB FAN - Equipped with a quiet rifle bearing, the 7-blade Air Balance 2.0 fan delivers higher air pressure (2.5 mmH2O) with minimal noise (27 dBA). Its reinforced frame enhances overall durability.  RGB MOTHERBOARD SYNC OR WIRED CONTROL - Compatible with RGB motherboard systems (4-pin) or manually controlled with the included wired controller and 3-to-1 splitter. |